**REQUEST FOR PROPOSAL**

**GENERAL CONTRACTOR**

**WILL ROGERS BIRTHPLACE RANCH**

**BIRTHPLACE HOME RESTORATION**

**ADDENDUM 1**

**December 12, 2024**

1. **Bid date has been extended to December 20th at 12PM**.

**Question & Answer Log for questions submitted prior to deadline:**

* + - 1. East and west doors are pre-hung with pre-primed finger jointed jamb, which are prone to rot. Do you want these two doors to be specified as doors and jambs in specified material?

**Replace exterior doors and jambs with either 1and 1/2 inch or 1 and 3/4 doors and jambs.**

* + - 1. Front entry door has been replaced previously with the incorrect size. It was altered from an 82" door to an 80", which has caused the sight line across the tops of the sidelites and door to be off by ~2" and a non-historic exterior casing to be added to the front side of the transom sill. Should this door jamb be replaced with a historically appropriate door size?

**Yes replace door with appropriate historical door**

* + - 1. Configuration: Window over two panel match existing exterior Second Floor Sleeping Porch Historic door

**Match the figure 1 except revise to show 6 panels in lieu of the 4 shown**.

* + - 1. The existing door on the sleeping porch has the mortises to indicate it a 6 lite over the 2 panels

**Match the figure 1 except revise to show 6 panels in lieu of the 4 shown**

* + - 1. The center muntin is larger with smaller horizontal muntins that would have resembled the last attached photo, except with 6 lites instead of 4 in the photo.

**Match the figure 1 photo except revise to show 6 panels in lieu of the 4 shown**

* + - 1. How would you like to proceed with all door configurations?

**Match the figure 1 photo except revise to show 6 panels in lieu of the 4 shown**

Figure 1

**-END OF ADDENDUM 1-**