**Specifications for WhisperRoom Sound Isolation Enclosure**

* 8.5’ x 14’ Enhanced (E), Double Wall Isolation Item #MDL 102168 E
* Standard Ventilation Systems (4)
* Interior Duct Covers (10)
* Wireless Remote (1)
* Cable Passages (8)
* StudioFoam (9-2’x4’ sheets)
* Wide Access Upgrade #WA UPG ENH 40
* Door Window (16’x48”)
* Hinge Preference- Left
* Gray Audimute Panels- 2 panels 2’x4’
* 4 Exterior Fan Silencer Boxes #EFS 102168
* 4-52” Studio Lights #SL 102168
* Ventilation Silencing System #VSS 102168
* Enhanced Window (26” x 48”)
* Two Bass Traps w/Velcro #BASS TRAPS

**PLEASE PROVIDE A LEAD TIME ON THE WHISPERROOM**