SPECIFICATION SHEET RFP

One **CLARK SE15 3-WHEELED SIT-DOWN RIDER**

o 3,000-pound Capacity at a 24” Load Center

o 188” Triple Stage Mast

o Side Shifter

o 42” Long Forks

o Cushion Tires (Warehouse / Concrete / Pavement)

o 36-Volts

o 2 -LED Headlights

o Safety Light

o Strobe Light

o Convenience Console

o 5” LCD Display

o Rear Grab Handle with Horn

o 12-Volt Convertor

o USB Port

o Back-Up Alarm

o Full Suspension Seat

o Delivery Included

New Warranty:

2-years / 4,000-hours

3-years / 6,000-hours

**Battery & Charger Options:**

**Lead Acid Package**

Battery & Charger with Watering System

5-Year Warranty

Battery Maintenance Required

**Lithium Package**

Battery & Charger

10-Year Warranty

5-Years Monitoring System Included

No Maintenance Required